{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Ballastberechnung"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Ballastberechnung","index":0,"n_rows":55,"n_cols":17,"rows_kept":55,"flags":["formulas_cached_only"]}
[]
[null,null,"Needle 124 - Ballastierung und Schwerpunktverschiebung"]
[]
[]
[null,null,"gilt nur bei den 124er mit den Ballastkammern wie angegeben - hinten 30mm breit"]
{"$rows_empty":9}
[{"$nulls":5},1.25,null,2.5,1.25]
[]
[{"$nulls":3},45,null,null,66.75,null,84.25,{"$nulls":3},112]
[null,null,"Ballastkammer vorne",{"$nulls":3},"Flügel-","Verbinder",null,null,"Ballastkammer hinten"]
[]
[null,null,34,56]
[{"$nulls":5},58,null,75.5,93,null,"96mm",null,null,128]
[]
[]
[]
[null,null,"gelbe Felder können geändert werden"]
[]
[]
[null,null,"gedachter Schwerpunkt Ballast bei mm",null,null,91]
[{"$nulls":7},"mm","Ballast in g",{"$nulls":4},"Ballast ges.","Stck.","Ballast je Stck."]
[null,null,"Entfernung \"Mitte\" hintere Flügelballastkammer zum Schwerpunkt:",{"$nulls":4},21,1224,null,"hinten",null,null,1224,16,{"v":76.5,"d":"76.50"}]
[null,null,"Entfernung \"Mitte\" hintere Verbinderballastkammer zum Schwerpunkt:",{"$nulls":4},6.75,{"$nulls":6},"li + re zusammen"]
[null,null,"Entfernung \"Mitte\" vordere Verbinderballastkammer zum Schwerpunkt:",{"$nulls":4},24.25]
[null,null,"Entfernung \"Mitte\" vordere Flügelballastkammer zum Schwerpunkt:",{"$nulls":4},46,{"$nulls":6},"          sollte gleich sein"]
[]
[{"$nulls":13},"Ballast ges.","Stck.","Ballast je Stck."]
[null,null,"Ausgleichsballast vordere Flügelballastkammer",{"$nulls":5},{"v":558.7826086956521,"d":"558.8"},null,"vorne",null,null,{"v":558.7826086956521,"d":"558.8"},{"v":16.001792917974,"d":"16.00"},34.92,"Gewicht ändern bis"]
[{"$nulls":14},"li + re zusammen",null,"Stückzahl gleich mit hinten"]
[{"$nulls":6},"Maximale Zuladung",null,{"v":1782.782608695652,"d":"1783"}]
[{"$nulls":13},"wenn Ballast vorne \"minus\""]
[{"$nulls":13},"gedachten Schwerpunkt ändern"]
[]
[]
[]
[]
[null,null,"Gewicht leer",null,"Schwerpunkt leer",null,"Schwerpunkt Ballast",null,"Schwerpunkt gesamt"]
[]
[null,null,2390,null,91,null,91,null,{"v":91,"d":"91.000"}]
[]
[]
[]
[]
[]
[null,"Version 1.2"]
[null,"09.09.2013"]
[null,"RG"]